- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

# compiler.h File Reference

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
union | Union32
union | Union16
## Defines
#define | LITTLE_ENDIAN
#define | PASS 0
#define | FAIL 1
#define | _MEM_TYPE_BIT_
#define | _MEM_TYPE_FAST_
#define | _MEM_TYPE_MEDFAST_
#define | _MEM_TYPE_MEDSLOW_
#define | _MEM_TYPE_SLOW_
#define | INTEL_ALIGNMENT LITTLE_ENDIAN
#define | MOTOROLA_ALIGNMENT BIG_ENDIAN
#define | MSB(u16) (((U8* )&u16)[1])
#define | LSB(u16) (((U8* )&u16)[0])
#define | MSW(u32) (((U16*)&u32)[1])
#define | LSW(u32) (((U16*)&u32)[0])
#define | MSB0(u32) (((U8* )&u32)[3])
#define | MSB1(u32) (((U8* )&u32)[2])
#define | MSB2(u32) (((U8* )&u32)[1])
#define | MSB3(u32) (((U8* )&u32)[0])
#define | LSB0(u32) MSB3(u32)
#define | LSB1(u32) MSB2(u32)
#define | LSB2(u32) MSB1(u32)
#define | LSB3(u32) MSB0(u32)
#define | Le16(b)
#define | Le32(b)
#define | htons(a) Le16(a)
#define | ntohs(a) htons(a)
#define | htonl(a) Le32(a)
#define | ntohl(a) htonl(a)
#define | ENABLE 1
#define | ENABLED 1
#define | DISABLED 0
#define | DISABLE 0
#define | FALSE (0==1)
#define | TRUE (1==1)
#define | KO 0
#define | OK 1
#define | OFF 0
#define | ON 1
#define | NULL 0
#define | CLR 0
#define | SET 1
#define | LOW(U16) ((Uchar)U16)
#define | HIGH(U16) ((Uchar)(U16>>8))
#define | TST_BIT_X(addrx, mask) (*addrx & mask)
#define | SET_BIT_X(addrx, mask) (*addrx = (*addrx | mask))
#define | CLR_BIT_X(addrx, mask) (*addrx = (*addrx & ~mask))
#define | OUT_X(addrx, value) (*addrx = value)
#define | IN_X(addrx) (*addrx)
#define | Max(a, b) ( (a)>(b) ? (a) : (b) )
#define | Min(a, b) ( (a)<(b) ? (a) : (b) )
#define | Upper(val, n) ( ((val)+(n)) & ~((n)-1) )
#define | Align_up(val, n) ( ((val)+(n)-1) & ~((n)-1) )
#define | Align_down(val, n) ( (val) & ~((n)-1) )
#define | Long_call(addr) ((*(void (_ConstType_*)(void))(addr))())
#define | SET_SFR_BIT(sfr_reg, bit_pos, bit_val) { sfr_reg &= ~(1<<(bit_pos)); sfr_reg |= ((bit_val)<<(bit_pos));}
#define | bit_is_clear(PORT, POSITION) ((PORT & (1<<POSITION)) == 0 )
#define | bit_is_set(PORT, POSITION) ((PORT & (1<<POSITION)) != 0 )
#define | __IOMACRO_H
#define | TID_GUARD(proc) ((__TID__ & 0x7FF0) != ((90 << 8) | ((proc) << 4)))
#define | SFR_B(_NAME, _ADDR)
#define | SFR_B2(_NAME1, _NAME2, _ADDR)
#define | SFR_B_EXT(_NAME, _ADDR)
#define | SFR_W(_NAME, _ADDR)
#define | SFR_W_EXT(_NAME, _ADDR)
## Typedefs
typedef float | Float16
typedef unsigned char | U8
typedef unsigned short | U16
typedef unsigned long | U32
typedef signed char | S8
typedef signed short | S16
typedef long | S32
typedef unsigned char | Bool
typedef U8 | Status
typedef Bool | Status_bool
typedef unsigned char | Uchar
typedef unsigned char | Uint8
typedef unsigned int | Uint16
typedef unsigned long int | Uint32
typedef char | Int8
typedef int | Int16
typedef long int | Int32
typedef unsigned char | Byte
typedef unsigned int | Word
typedef unsigned long int | DWord
typedef char | p_uart_ptchar
typedef char | r_uart_ptchar

## Define Documentation

#define LITTLE_ENDIAN

Definition at line 22 of file compiler.h.

#define PASS 0

Definition at line 41 of file compiler.h.

#define FAIL 1

Definition at line 42 of file compiler.h.

#define _MEM_TYPE_BIT_

Definition at line 53 of file compiler.h.

#define _MEM_TYPE_FAST_

Definition at line 54 of file compiler.h.

#define _MEM_TYPE_MEDFAST_

Definition at line 55 of file compiler.h.

#define _MEM_TYPE_MEDSLOW_

Definition at line 56 of file compiler.h.

#define _MEM_TYPE_SLOW_

Definition at line 57 of file compiler.h.

Referenced by sbc_read_capacity().

#define INTEL_ALIGNMENT LITTLE_ENDIAN

Definition at line 157 of file compiler.h.

#define MOTOROLA_ALIGNMENT BIG_ENDIAN

Definition at line 158 of file compiler.h.

#define MSB | ( | u16 |  | ) | (((U8* )&u16)[1])

Definition at line 162 of file compiler.h.

Referenced by hid_get_hid_descriptor(), hid_get_report(), sbc_read_10(), sbc_write_10(), usb_get_descriptor(), usb_hid_get_interface(), and usb_hid_set_idle().

#define LSB | ( | u16 |  | ) | (((U8* )&u16)[0])

Definition at line 163 of file compiler.h.

Referenced by hid_get_hid_descriptor(), hid_get_report(), sbc_read_10(), sbc_write_10(), usb_get_descriptor(), usb_hid_get_interface(), and usb_hid_set_idle().

#define MSW | ( | u32 |  | ) | (((U16*)&u32)[1])

Definition at line 164 of file compiler.h.

#define LSW | ( | u32 |  | ) | (((U16*)&u32)[0])

Definition at line 165 of file compiler.h.

#define MSB0 | ( | u32 |  | ) | (((U8* )&u32)[3])

Definition at line 166 of file compiler.h.

Referenced by sbc_read_10(), sbc_read_capacity(), and sbc_write_10().

#define MSB1 | ( | u32 |  | ) | (((U8* )&u32)[2])

Definition at line 167 of file compiler.h.

Referenced by df_read_open(), df_write_open(), sbc_read_10(), sbc_read_capacity(), and sbc_write_10().

#define MSB2 | ( | u32 |  | ) | (((U8* )&u32)[1])

Definition at line 168 of file compiler.h.

Referenced by df_read_open(), df_read_sector(), df_write_close(), df_write_open(), df_write_sector(), sbc_read_10(), sbc_read_capacity(), and sbc_write_10().

#define MSB3 | ( | u32 |  | ) | (((U8* )&u32)[0])

Definition at line 169 of file compiler.h.

Referenced by df_read_open(), df_write_close(), df_write_open(), sbc_read_10(), sbc_read_capacity(), and sbc_write_10().

#define LSB0 | ( | u32 |  | ) | MSB3(u32)

Definition at line 170 of file compiler.h.

Referenced by df_read_10(), df_read_open(), df_write_10(), df_write_open(), and usb_mass_storage_cbw().

#define LSB1 | ( | u32 |  | ) | MSB2(u32)

Definition at line 171 of file compiler.h.

Referenced by usb_mass_storage_cbw().

#define LSB2 | ( | u32 |  | ) | MSB1(u32)

Definition at line 172 of file compiler.h.

Referenced by usb_mass_storage_cbw().

#define LSB3 | ( | u32 |  | ) | MSB0(u32)

Definition at line 173 of file compiler.h.

Referenced by usb_mass_storage_cbw().

#define Le16 | ( | b |  | ) |

Value:

    (  ((U16)(     (b) &   0xFF) << 8)  \
       |  (     ((U16)(b) & 0xFF00) >> 8)  \
       )

Definition at line 190 of file compiler.h.

#define Le32 | ( | b |  | ) |

Value:

    (  ((U32)(     (b) &       0xFF) << 24)  \
       |  ((U32)((U16)(b) &     0xFF00) <<  8)  \
       |  (     ((U32)(b) &   0xFF0000) >>  8)  \
       |  (     ((U32)(b) & 0xFF000000) >> 24)  \
       )

Definition at line 194 of file compiler.h.

#define htons | ( | a |  | ) | Le16(a)

Definition at line 206 of file compiler.h.

#define ntohs | ( | a |  | ) | htons(a)

Definition at line 207 of file compiler.h.

#define htonl | ( | a |  | ) | Le32(a)

Definition at line 208 of file compiler.h.

#define ntohl | ( | a |  | ) | htonl(a)

Definition at line 209 of file compiler.h.

#define ENABLE 1

Definition at line 219 of file compiler.h.

#define ENABLED 1

Definition at line 220 of file compiler.h.

Referenced by usb_clear_feature(), and usb_set_feature().

#define DISABLED 0

Definition at line 221 of file compiler.h.

Referenced by usb_clear_feature(), usb_general_interrupt(), and usb_task_init().

#define DISABLE 0

Definition at line 222 of file compiler.h.

#define FALSE (0==1)

Definition at line 223 of file compiler.h.

Referenced by df_read_sector(), df_removal(), df_wr_protect(), df_write_sector(), hid_get_hid_descriptor(), hid_get_report(), is_usb_mouse_event(), sbc_inquiry(), sbc_mode_sense(), sbc_read_10(), sbc_read_capacity(), sbc_write_10(), scsi_decode_command(), usb_device_task(), usb_get_descriptor(), usb_init_device(), usb_mass_storage_cbw(), usb_process_request(), usb_user_get_descriptor(), and usb_user_read_request().

#define TRUE (1==1)

Definition at line 224 of file compiler.h.

Referenced by hid_get_hid_descriptor(), hid_get_report(), is_usb_mouse_event(), mouse_task_by_IT(), mouse_task_init(), sbc_inquiry(), sbc_mode_sense(), sbc_prevent_allow_medium_removal(), sbc_read_10(), sbc_read_capacity(), sbc_request_sense(), sbc_test_unit_ready(), sbc_write_10(), scsi_decode_command(), spi_init(), usb_device_task(), usb_get_descriptor(), usb_mass_storage_cbw(), usb_user_get_descriptor(), and usb_user_read_request().

#define KO 0

Definition at line 226 of file compiler.h.

Referenced by df_mem_check().

#define OK 1

Definition at line 227 of file compiler.h.

Referenced by df_init(), df_mem_check(), df_read_open(), df_read_sector(), df_read_sector_2_ram(), df_test_unit_ready(), df_write_open(), df_write_sector(), and df_write_sector_from_ram().

#define OFF 0

Definition at line 228 of file compiler.h.

#define ON 1

Definition at line 229 of file compiler.h.

#define NULL 0

Definition at line 231 of file compiler.h.

Referenced by df_format().

#define CLR 0

Definition at line 234 of file compiler.h.

#define SET 1

Definition at line 235 of file compiler.h.

#define LOW | ( | U16 |  | ) | ((Uchar)U16)

Definition at line 239 of file compiler.h.

#define HIGH | ( | U16 |  | ) | ((Uchar)(U16>>8))

Definition at line 240 of file compiler.h.

#define TST_BIT_X | ( | addrx,
|  | mask |  | ) | (*addrx & mask)

Definition at line 241 of file compiler.h.

#define SET_BIT_X | ( | addrx,
|  | mask |  | ) | (*addrx = (*addrx | mask))

Definition at line 242 of file compiler.h.

#define CLR_BIT_X | ( | addrx,
|  | mask |  | ) | (*addrx = (*addrx & ~mask))

Definition at line 243 of file compiler.h.

#define OUT_X | ( | addrx,
|  | value |  | ) | (*addrx = value)

Definition at line 244 of file compiler.h.

#define IN_X | ( | addrx |  | ) | (*addrx)

Definition at line 245 of file compiler.h.

#define Max | ( | a,
|  | b |  | ) | ( (a)>(b) ? (a) : (b) )

Definition at line 247 of file compiler.h.

#define Min | ( | a,
|  | b |  | ) | ( (a)<(b) ? (a) : (b) )

Definition at line 248 of file compiler.h.

#define Upper | ( | val,
|  | n |  | ) | ( ((val)+(n)) & ~((n)-1) )

Definition at line 257 of file compiler.h.

#define Align_up | ( | val,
|  | n |  | ) | ( ((val)+(n)-1) & ~((n)-1) )

Definition at line 266 of file compiler.h.

#define Align_down | ( | val,
|  | n |  | ) | ( (val) & ~((n)-1) )

Definition at line 275 of file compiler.h.

#define Long_call | ( | addr |  | ) | ((*(void (_ConstType_*)(void))(addr))())

Definition at line 292 of file compiler.h.

#define SET_SFR_BIT | ( | sfr_reg,
|  | bit_pos,
|  | bit_val |  | ) | { sfr_reg &= ~(1<<(bit_pos)); sfr_reg |= ((bit_val)<<(bit_pos));}

Definition at line 304 of file compiler.h.

#define bit_is_clear | ( | PORT,
|  | POSITION |  | ) | ((PORT & (1<<POSITION)) == 0 )

Definition at line 314 of file compiler.h.

#define bit_is_set | ( | PORT,
|  | POSITION |  | ) | ((PORT & (1<<POSITION)) != 0 )

Definition at line 324 of file compiler.h.

#define __IOMACRO_H

Definition at line 332 of file compiler.h.

#define TID_GUARD | ( | proc |  | ) | ((__TID__ & 0x7FF0) != ((90 << 8) | ((proc) << 4)))

Definition at line 334 of file compiler.h.

#define SFR_B | ( | _NAME,
|  | _ADDR |  | ) |

Value:

    SFR_B_BITS(_NAME, _ADDR, \
                                        Bit0,Bit1,Bit2,Bit3,Bit4,Bit5,Bit6,Bit7)

Definition at line 445 of file compiler.h.

#define SFR_B2 | ( | _NAME1,
|  | _NAME2,
|  | _ADDR |  | ) |

Value:

    SFR_B2_BITS(_NAME1, _NAME2, _ADDR, \
                                        Bit0,Bit1,Bit2,Bit3,Bit4,Bit5,Bit6,Bit7)

Definition at line 447 of file compiler.h.

#define SFR_B_EXT | ( | _NAME,
|  | _ADDR |  | ) |

Value:

    SFR_B_BITS_EXT(_NAME, _ADDR, \
                                        Bit0,Bit1,Bit2,Bit3,Bit4,Bit5,Bit6,Bit7)

Definition at line 449 of file compiler.h.

#define SFR_W | ( | _NAME,
|  | _ADDR |  | ) |

Value:

    SFR_W_BITS(_NAME, _ADDR, \
                                        Bit0,Bit1,Bit2,Bit3,Bit4,Bit5,Bit6,Bit7, \
                                        Bit8,Bit9,Bit10,Bit11,Bit12,Bit13,Bit14,Bit15)

Definition at line 452 of file compiler.h.

#define SFR_W_EXT | ( | _NAME,
|  | _ADDR |  | ) |

Value:

    SFR_W_BITS_EXT(_NAME, _ADDR, \
                                        Bit0,Bit1,Bit2,Bit3,Bit4,Bit5,Bit6,Bit7, \
                                        Bit8,Bit9,Bit10,Bit11,Bit12,Bit13,Bit14,Bit15)

Definition at line 456 of file compiler.h.

## Typedef Documentation

typedef float Float16

Definition at line 25 of file compiler.h.

typedef unsigned char U8

Definition at line 27 of file compiler.h.

typedef unsigned short U16

Definition at line 28 of file compiler.h.

typedef unsigned long U32

Definition at line 29 of file compiler.h.

typedef signed char S8

Definition at line 30 of file compiler.h.

typedef signed short S16

Definition at line 31 of file compiler.h.

typedef long S32

Definition at line 32 of file compiler.h.

typedef unsigned char Bool

Definition at line 36 of file compiler.h.

typedef U8 Status

Definition at line 39 of file compiler.h.

typedef Bool Status_bool

Definition at line 40 of file compiler.h.

typedef unsigned char Uchar

Definition at line 60 of file compiler.h.

typedef unsigned char Uint8

Definition at line 63 of file compiler.h.

typedef unsigned int Uint16

Definition at line 64 of file compiler.h.

typedef unsigned long int Uint32

Definition at line 65 of file compiler.h.

typedef char Int8

Definition at line 67 of file compiler.h.

typedef int Int16

Definition at line 68 of file compiler.h.

typedef long int Int32

Definition at line 69 of file compiler.h.

typedef unsigned char Byte

Definition at line 71 of file compiler.h.

typedef unsigned int Word

Definition at line 72 of file compiler.h.

typedef unsigned long int DWord

Definition at line 73 of file compiler.h.

typedef char p_uart_ptchar

Definition at line 99 of file compiler.h.

typedef char r_uart_ptchar

Definition at line 100 of file compiler.h.