- Main Page
- Modules
- Data Structures
- Files
- Related Pages

- File List
- Globals

# ctrl_status.h File Reference

Copyright (c) 2004This file contains the interface :

- between USB <-> MEMORY OR
- between USB <- Access Memory Ctrl -> Memory.

More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Enumerations
enum | Ctrl_status { CTRL_GOOD = (PASS ), CTRL_FAIL = (FAIL ), CTRL_NO_PRESENT = (FAIL+1), CTRL_BUSY = (FAIL+2) }
| Define control status. More...

## Detailed Description

Copyright (c) 2004This file contains the interface :

- between USB <-> MEMORY OR
- between USB <- Access Memory Ctrl -> Memory.

Please read file license.txt for copyright notice.

This interface may be controled by a "Access Memory Control" for :

- include a management of write protect global or specific
- include a management of access password
- ...

Version:
  1.1 (c5131-mass-storage-virtual-1_0_4)

Todo:

Bug:

Definition in file ctrl_status.h.

## Enumeration Type Documentation

enum Ctrl_status

Define control status.

Enumerator:

  CTRL_GOOD |
  CTRL_FAIL |
  CTRL_NO_PRESENT |
  CTRL_BUSY |

Definition at line 29 of file ctrl_status.h.

    00030 {
    00031    CTRL_GOOD         =(PASS  )  // It is ready
    00032 ,  CTRL_FAIL         =(FAIL  )  // Memory fail
    00033 ,  CTRL_NO_PRESENT   =(FAIL+1)  // Memory unplug
    00034 ,  CTRL_BUSY         =(FAIL+2)  // Not initialize
    00035 } Ctrl_status;